Static Call Graph - [.\STM32-DEMO.axf]

# Static Call Graph for image .\STM32-DEMO.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Mon Nov 24 23:03:50 2014

### Maximum Stack Usage = 152 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ OSInit ⇒ OSTaskCreateExt ⇒ OS_TCBInit

### Functions with no stack information

- OS_CPU_SR_Save
- OS_CPU_SR_Restore
- OSStartHighRdy
- OSCtxSw
- OSIntCtxSw
- OS_CPU_PendSVHandler

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - OSTaskSwHook from os_cpu_c.o(.text) referenced from os_cpu_a.o(.text)
  - OS_CPU_PendSVHandler from os_cpu_a.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - OS_TaskIdle from os_core.o(.text) referenced from os_core.o(.text)
  - OS_TaskStat from os_core.o(.text) referenced from os_core.o(.text)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit_ExtMemCtl from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Task_LED2 from app.o(.text) referenced from app.o(.text)
  - Task_Start from app.o(.text) referenced from main.o(.text)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_hd.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  SystemInit_ExtMemCtl (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  Reset_Handler (Thumb, 14 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  main (Thumb, 30 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = main ⇒ OSInit ⇒ OSTaskCreateExt ⇒ OS_TCBInit
  [Calls]
  - >> OSTaskCreate
  - >> OSStart
  - >> OSInit
  - >> BSP_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  SysTick_Handler (Thumb, 18 bytes, Stack size 8 bytes, stm32f10x_it.o(.text))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = SysTick_Handler ⇒ OSTimeTick
  [Calls]
  - >> OSTimeTick
  - >> OSIntExit
  - >> OSIntEnter
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  GPIO_DeInit (Thumb, 152 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 152 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> LED_GPIO_Config

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LED_GPIO_Config
  - >> Task_Start

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> Task_Start

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 42 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 130 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_AHBPeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> LED_GPIO_Config

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  SystemInit (Thumb, 48 bytes, Stack size 0 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SystemInit ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> BSP_Init

  BSP_Init (Thumb, 14 bytes, Stack size 8 bytes, bsp.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = BSP_Init ⇒ LED_GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> LED_GPIO_Config
  - >> SystemInit
  [Called By]
  - >> main

  SysTick_init (Thumb, 46 bytes, Stack size 0 bytes, bsp.o(.text))
  [Called By]

  - >> Task_LED2
  - >> Task_Start

  LED_GPIO_Config (Thumb, 50 bytes, Stack size 16 bytes, led.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LED_GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> BSP_Init

  Task_LED2 (Thumb, 34 bytes, Stack size 0 bytes, app.o(.text))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = Task_LED2 ⇒ OSTimeDlyHMSM ⇒ OSTimeDly ⇒ OS_Sched
  [Calls]
  - >> OSTimeDlyHMSM
  - >> SysTick_init
  [Address Reference Count : 1]
  - app.o(.text)

  Task_Start (Thumb, 66 bytes, Stack size 0 bytes, app.o(.text))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = Task_Start ⇒ OSTaskCreate ⇒ OS_TCBInit
  [Calls]
  - >> OSTimeDlyHMSM
  - >> SysTick_init
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> OSTaskCreate
  [Address Reference Count : 1]
  - main.o(.text)

  OS_StrCopy (Thumb, 28 bytes, Stack size 0 bytes, os_core.o(.text))
  [Called By]

  - >> OSTaskNameGet
  - >> OSTaskNameSet
  - >> OSEventNameSet
  - >> OSEventNameGet

  OSEventNameGet (Thumb, 96 bytes, Stack size 24 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_StrCopy

  OS_StrLen (Thumb, 20 bytes, Stack size 0 bytes, os_core.o(.text))
  [Called By]

  - >> OSTaskNameSet
  - >> OSEventNameSet

  OSEventNameSet (Thumb, 106 bytes, Stack size 24 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_StrLen
  - >> OS_StrCopy

  OS_TaskStatStkChk (Thumb, 50 bytes, Stack size 24 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = OS_TaskStatStkChk ⇒ OSTaskStkChk
  [Calls]
  - >> OSTaskStkChk
  [Called By]
  - >> OS_TaskStat

  OS_TaskStat (Thumb, 82 bytes, Stack size 0 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = OS_TaskStat ⇒ OS_TaskStatStkChk ⇒ OSTaskStkChk
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSTimeDly
  - >> OSTaskSuspend
  - >> OSTaskStatHook
  - >> OS_TaskStatStkChk
  [Address Reference Count : 1]
  - os_core.o(.text)

  OS_TaskIdle (Thumb, 22 bytes, Stack size 0 bytes, os_core.o(.text))
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSTaskIdleHook
  [Address Reference Count : 1]
  - os_core.o(.text)

  OS_MemClr (Thumb, 18 bytes, Stack size 0 bytes, os_core.o(.text))
  [Called By]

  - >> OSInit

  OSInit (Thumb, 282 bytes, Stack size 40 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = OSInit ⇒ OSTaskCreateExt ⇒ OS_TCBInit
  [Calls]
  - >> OSTaskNameSet
  - >> OSTaskCreateExt
  - >> OSInitHookEnd
  - >> OSInitHookBegin
  - >> OS_MemClr
  [Called By]
  - >> main

  OSIntEnter (Thumb, 20 bytes, Stack size 0 bytes, os_core.o(.text))
  [Called By]

  - >> SysTick_Handler

  OSIntExit (Thumb, 82 bytes, Stack size 16 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = OSIntExit
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSIntCtxSw
  - >> OS_SchedNew
  [Called By]
  - >> SysTick_Handler

  OSSchedLock (Thumb, 38 bytes, Stack size 8 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore

  OS_Sched (Thumb, 64 bytes, Stack size 16 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = OS_Sched
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSCtxSw
  - >> OS_SchedNew
  [Called By]
  - >> OSTimeDlyResume
  - >> OSTaskResume
  - >> OSTaskDel
  - >> OSTaskChangePrio
  - >> OSTimeDly
  - >> OSTaskSuspend
  - >> OSTaskCreateExt
  - >> OSSchedUnlock
  - >> OSTaskCreate

  OSSchedUnlock (Thumb, 52 bytes, Stack size 8 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched

  OSStart (Thumb, 38 bytes, Stack size 8 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = OSStart
  [Calls]
  - >> OSStartHighRdy
  - >> OS_SchedNew
  [Called By]
  - >> main

  OSStatInit (Thumb, 102 bytes, Stack size 8 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSTimeDly

  OSTimeTick (Thumb, 158 bytes, Stack size 24 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = OSTimeTick
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSTimeTickHook
  [Called By]
  - >> SysTick_Handler

  OSVersion (Thumb, 6 bytes, Stack size 0 bytes, os_core.o(.text), UNUSED)

  OS_Dummy (Thumb, 2 bytes, Stack size 0 bytes, os_core.o(.text), UNUSED)
  [Called By]

  - >> OSTaskDel

  OS_EventTaskRemove (Thumb, 32 bytes, Stack size 8 bytes, os_core.o(.text), UNUSED)
  [Called By]

  - >> OSTaskDel
  - >> OS_EventTaskRdy

  OS_EventTaskRdy (Thumb, 88 bytes, Stack size 16 bytes, os_core.o(.text), UNUSED)
  [Calls]

  - >> OS_EventTaskRemove

  OS_EventTaskWait (Thumb, 66 bytes, Stack size 12 bytes, os_core.o(.text), UNUSED)

  OS_EventWaitListInit (Thumb, 22 bytes, Stack size 0 bytes, os_core.o(.text), UNUSED)

  OS_MemCopy (Thumb, 20 bytes, Stack size 0 bytes, os_core.o(.text), UNUSED)
  [Called By]

  - >> OSTaskQuery

  OS_TCBInit (Thumb, 204 bytes, Stack size 40 bytes, os_core.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = OS_TCBInit
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OSTaskCreateHook
  - >> OSTCBInitHook
  [Called By]
  - >> OSTaskCreateExt
  - >> OSTaskCreate

  OSTaskChangePrio (Thumb, 276 bytes, Stack size 40 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched

  OSTaskCreate (Thumb, 132 bytes, Stack size 40 bytes, os_task.o(.text))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = OSTaskCreate ⇒ OS_TCBInit
  [Calls]
  - >> OSTaskStkInit
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_TCBInit
  - >> OS_Sched
  [Called By]
  - >> Task_Start
  - >> main

  OS_TaskStkClr (Thumb, 22 bytes, Stack size 0 bytes, os_task.o(.text))
  [Called By]

  - >> OSTaskCreateExt

  OSTaskCreateExt (Thumb, 152 bytes, Stack size 64 bytes, os_task.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = OSTaskCreateExt ⇒ OS_TCBInit
  [Calls]
  - >> OSTaskStkInit
  - >> OS_TaskStkClr
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_TCBInit
  - >> OS_Sched
  [Called By]
  - >> OSInit

  OSTaskDel (Thumb, 268 bytes, Stack size 32 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OSTaskDelHook
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_EventTaskRemove
  - >> OS_Dummy
  - >> OS_Sched

  OSTaskDelReq (Thumb, 88 bytes, Stack size 8 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore

  OSTaskNameGet (Thumb, 154 bytes, Stack size 24 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_StrCopy

  OSTaskNameSet (Thumb, 130 bytes, Stack size 24 bytes, os_task.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = OSTaskNameSet
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_StrLen
  - >> OS_StrCopy
  [Called By]
  - >> OSInit

  OSTaskResume (Thumb, 126 bytes, Stack size 8 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched

  OSTaskStkChk (Thumb, 126 bytes, Stack size 24 bytes, os_task.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = OSTaskStkChk
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  [Called By]
  - >> OS_TaskStatStkChk

  OSTaskSuspend (Thumb, 148 bytes, Stack size 16 bytes, os_task.o(.text))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = OSTaskSuspend ⇒ OS_Sched
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched
  [Called By]
  - >> OS_TaskStat

  OSTaskQuery (Thumb, 94 bytes, Stack size 16 bytes, os_task.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_MemCopy

  OSTimeDly (Thumb, 74 bytes, Stack size 16 bytes, os_time.o(.text))
  [Stack]

  - Max Depth = 32 + Unknown Stack Size
  - Call Chain = OSTimeDly ⇒ OS_Sched
  [Calls]
  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched
  [Called By]
  - >> OSStatInit
  - >> OS_TaskStat
  - >> OSTimeDlyHMSM

  OSTimeDlyHMSM (Thumb, 128 bytes, Stack size 16 bytes, os_time.o(.text))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = OSTimeDlyHMSM ⇒ OSTimeDly ⇒ OS_Sched
  [Calls]
  - >> OSTimeDly
  [Called By]
  - >> Task_LED2
  - >> Task_Start

  OSTimeDlyResume (Thumb, 132 bytes, Stack size 8 bytes, os_time.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore
  - >> OS_Sched

  OSTimeGet (Thumb, 18 bytes, Stack size 8 bytes, os_time.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore

  OSTimeSet (Thumb, 20 bytes, Stack size 8 bytes, os_time.o(.text), UNUSED)
  [Calls]

  - >> OS_CPU_SR_Save
  - >> OS_CPU_SR_Restore

  OS_CPU_SR_Save (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Called By]

  - >> OSTimeSet
  - >> OSTimeGet
  - >> OSTimeDlyResume
  - >> OSTaskQuery
  - >> OSTaskResume
  - >> OSTaskNameGet
  - >> OSTaskDelReq
  - >> OSTaskDel
  - >> OSTaskChangePrio
  - >> OSTimeDly
  - >> OSTaskSuspend
  - >> OSTaskStkChk
  - >> OSTaskNameSet
  - >> OSTaskCreateExt
  - >> OS_TCBInit
  - >> OSStatInit
  - >> OSSchedUnlock
  - >> OS_Sched
  - >> OSSchedLock
  - >> OS_TaskIdle
  - >> OS_TaskStat
  - >> OSEventNameSet
  - >> OSEventNameGet
  - >> OSTimeTick
  - >> OSIntExit
  - >> OSTaskCreate

  OS_CPU_SR_Restore (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Called By]

  - >> OSTimeSet
  - >> OSTimeGet
  - >> OSTimeDlyResume
  - >> OSTaskQuery
  - >> OSTaskResume
  - >> OSTaskNameGet
  - >> OSTaskDelReq
  - >> OSTaskDel
  - >> OSTaskChangePrio
  - >> OSTimeDly
  - >> OSTaskSuspend
  - >> OSTaskStkChk
  - >> OSTaskNameSet
  - >> OSTaskCreateExt
  - >> OS_TCBInit
  - >> OSStatInit
  - >> OSSchedUnlock
  - >> OS_Sched
  - >> OSSchedLock
  - >> OS_TaskIdle
  - >> OS_TaskStat
  - >> OSEventNameSet
  - >> OSEventNameGet
  - >> OSTimeTick
  - >> OSIntExit
  - >> OSTaskCreate

  OSStartHighRdy (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Called By]

  - >> OSStart

  OSCtxSw (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Called By]

  - >> OS_Sched

  OSIntCtxSw (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Called By]

  - >> OSIntExit

  OS_CPU_PendSVHandler (Thumb, 0 bytes, Stack size unknown bytes, os_cpu_a.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  OSInitHookBegin (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OSInit

  OSInitHookEnd (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OSInit

  OSTaskCreateHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OS_TCBInit

  OSTaskDelHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text), UNUSED)
  [Called By]

  - >> OSTaskDel

  OSTaskIdleHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OS_TaskIdle

  OSTaskStatHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OS_TaskStat

  OSTaskStkInit (Thumb, 114 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OSTaskCreateExt
  - >> OSTaskCreate

  OSTaskSwHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Address Reference Count : 1]

  - os_cpu_a.o(.text)

  OSTCBInitHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OS_TCBInit

  OSTimeTickHook (Thumb, 2 bytes, Stack size 0 bytes, os_cpu_c.o(.text))
  [Called By]

  - >> OSTimeTick

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClockTo72 (Thumb, 160 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SystemInit

  OS_SchedNew (Thumb, 24 bytes, Stack size 0 bytes, os_core.o(.text))
  [Called By]

  - >> OS_Sched
  - >> OSIntExit
  - >> OSStart

  ### Undefined Global Symbols