#

##

##

    礦ision Build Log
    Project:
    D:\BaiduYunDownload\STM32F103C8T6最小系统版资料\STM32_OLED(C8T6)\MDK-Proj\STM32_OLED.uvproj
    Project File Date:  10/22/2014

    Output:
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Failed!
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10444 RO-data=3300 RW-data=316 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    compiling stm32f10x_it.c...
    linking...
    .\STM32_OLED.axf: Error: L6218E: Undefined symbol Key1 (referred from stm32f10x_it.o).
    .\STM32_OLED.axf: Error: L6218E: Undefined symbol Key1_State (referred from stm32f10x_it.o).
    .\STM32_OLED.axf: Error: L6218E: Undefined symbol Key1_Value (referred from stm32f10x_it.o).
    .\STM32_OLED.axf: Error: L6218E: Undefined symbol WK_up_Key (referred from stm32f10x_it.o).
    ".\STM32_OLED.axf" - 4 Errors, 0 Warning(s).
    Target not created
    Build target 'STM32_OLED'
    compiling stm32f10x_it.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling BSP_Config.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling Eeprom.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=10364 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling BSP_Config.c...
    linking...
    Program Size: Code=10432 RO-data=3300 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    ..\APP\main.c(129): error:  #20: identifier "L_Buf" is undefined
    ..\APP\main.c(130): error:  #20: identifier "COM1_TxBuffer" is undefined
    ..\APP\main.c(130): error:  #20: identifier "NUM_Data" is undefined
    ..\APP\main.c(131): error:  #20: identifier "Data_buf" is undefined
    ".\STM32_OLED.axf" - 4 Errors, 0 Warning(s).
    Target not created
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12044 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12044 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=12060 RO-data=3820 RW-data=308 ZI-data=2404
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling send_DATA.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=11996 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12052 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12052 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12052 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12068 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Rebuild target 'STM32_OLED'
    compiling misc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    assembling startup_stm32f10x_md.s...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling BSP_Config.c...
    compiling send_DATA.c...
    compiling CRC.c...
    compiling oled.c...
    compiling Eeprom.c...
    linking...
    Program Size: Code=12068 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\STM32_OLED.axf"
    Include "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32_OLED(C8T6)\\MDK-Proj\\JLinkSettings.ini"
    [BREAKPOINTS]
    ^
    *** error 10: Syntax error
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    compiling main.c...
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).
    Build target 'STM32_OLED'
    linking...
    Program Size: Code=12056 RO-data=3820 RW-data=116 ZI-data=2212
    FromELF: creating hex file...
    ".\STM32_OLED.axf" - 0 Errors, 0 Warning(s).