#

##

##

    礦ision Build Log
    Project:
    D:\BaiduYunDownload\STM32F103C8T6最小系统版资料\STM32F103C8T6例程\基本例程-CRC操作\基本例程-CRC操作\CRC（循环冗余校验）\USER\STM32-DEMO.uvproj
    Project File Date:  03/01/2013

    Output:
    *** Note: 'Create Batch File' is active - using 'Rebuild'.
    Rebuild target 'CRC-DEMO'
    assembling startup_stm32f10x_hd.s...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling usart1.c...
    compiling crc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_crc.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    linking...
    Program Size: Code=4408 RO-data=792 RW-data=28 ZI-data=516
    FromELF: creating hex file...
    ".\STM32-DEMO.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32F103C8T6例程\\基本例程-CRC操作\\基本例程-CRC操作\\CRC（循环冗余校验）\\USER\\STM32-DEMO.axf"
    Erase Done.
    Programming Done.
    Verify OK.
    *** Note: 'Create Batch File' is active - using 'Rebuild'.
    Rebuild target 'CRC-DEMO'
    assembling startup_stm32f10x_hd.s...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling usart1.c...
    compiling crc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_crc.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    linking...
    Program Size: Code=4408 RO-data=792 RW-data=28 ZI-data=516
    FromELF: creating hex file...
    ".\STM32-DEMO.axf" - 0 Errors, 0 Warning(s).
    *** Note: 'Create Batch File' is active - using 'Rebuild'.
    Rebuild target 'CRC-DEMO'
    assembling startup_stm32f10x_hd.s...
    compiling main.c...
    compiling stm32f10x_it.c...
    compiling usart1.c...
    compiling crc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_crc.c...
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    linking...
    Program Size: Code=4408 RO-data=792 RW-data=28 ZI-data=516
    FromELF: creating hex file...
    ".\STM32-DEMO.axf" - 0 Errors, 0 Warning(s).
    Load "D:\\BaiduYunDownload\\STM32F103C8T6最小系统版资料\\STM32F103C8T6例程\\基本例程-CRC操作\\基本例程-CRC操作\\CRC（循环冗余校验）\\USER\\STM32-DEMO.axf"
    Erase Done.
    Programming Done.
    Verify OK.